LAMAX S7 Dual

Firmware update procedure

1. Format your micro SD card and copy "bin" file into root directory.
2. Insert micro SD card into camera and power on.
3. Camera will update automatically. Process of updating is displayed. 
4. After 100% finished, camera will power off automatically. 
5. Take out the micro SD card and format it on PC before using it again.

Important notification:

1. Copy installation file into root directory. Copying the file anywhere else causes the installation process will not start.
2. Remove the installation file from your micro SD card after installation process finish. Keeping the file on the card will cause re-start the installation process after inserting the card into your camera. 
3. Do not remove the card during installation process. It may cause damage to your microSD card or camera. Any claim will not be accepted in this case.
4. Camera must be plugged into a power supply during installation process. Switching off can cause damage of device.